---
title: "User's guide"
author: "Miquel De Cáceres, Victor Granda"
date: "`r Sys.Date()`"
output: 
  rmarkdown::html_vignette:
    toc: TRUE
vignette: >
  %\VignetteIndexEntry{User guide to meteoland}
  %\VignetteEngine{knitr::rmarkdown}
  %\VignetteEncoding{UTF-8}
---

```{r setup, include = FALSE}
knitr::opts_chunk$set(
  collapse = TRUE,
  comment = "#>"
)
library(meteoland)
```

# Introduction

## Purpose

Reliable meteorological data are a basic requirement for hydrological and ecological studies at the landscape scale. Given the large spatial variation of meteorology over complex terrains, meteorological records from a single weather station are often not representative of entire landscapes. Studies made on multiple sites over a landscape require different meteorological series for each site; and other studies may require meteorological data series for all grid cells of a landscape, in a continuous way. In these cases, spatial correlation between the meteorology series of different sites or cells must be taken into account. For example, the sequence of days with rain of contiguous cells will normally be the same or very similar, even if precipitation amounts may differ. Finally, studies addressing the impacts of climate change on forests and landscapes require downscaling coarse-scale predictions  of global or regional climate models to the landscape scale. When downscaling predictions for several locations in a landscape, spatial correlation of predictions is also important.

With the aim to assist research of climatic impacts on forests, the R package **meteoland** provides utilities to estimate daily weather variables at any position over complex terrains:

1. Spatial interpolation of daily weather records from meteorological stations. 
2. Statistical correction of meteorological data series (e.g. from climate models).
3. Multisite and multivariate stochastic weather generation.

Using **meteoland** package is easy, but some ideas and concepts must be addresed to make the experience easy for new users. This vignette is intended as a working example to explain all the steps needed to get comfortable with **meteoland** workflow. We assume that the reader is more or less familiar with S4 spatial classes of package [**sp**](https://cran.r-project.org/package=sp). You will find detailed information regarding the package structure, its functions, and how calculations are done at the [vegmod website](http://vegmod.ctfc.cat/software/meteoland/).

## Installing and loading the package

First of all, before starting to work with **meteoland**, we must install and load
the library. Stable versions of the package can be found at CRAN
(https://CRAN.R-project.org/package=meteoland), and it can be
installed and loaded as any other R package:

```{r, eval = FALSE}
install.packages("meteoland")
library(meteoland)
```

Alternatively, you can install the development version located at GitHub using the **devtools** package:
```{r, eval = FALSE}
library(devtools)
install_github("vegmod/meteoland", 
               build_opts = c("--no-resave-data", "--no-manual"))
library(meteoland)
```


# Interpolation of daily weather

Spatial interpolation is required when meteorology for the area and period of interest cannot be obtained from local sensors. The nearest weather station may not have data for the period of interest or it may be located too far away to be representative of the target area.

## Preparing weather data for interpolation


```{r, echo = FALSE, include= FALSE}
data("exampleinterpolationdata")

st_names = row.names(exampleinterpolationdata@MinTemperature)
st_coords = exampleinterpolationdata@coords
st_data = data.frame(X_UTM = st_coords[,1], Y_UTM = st_coords[,2],
                     elevation = exampleinterpolationdata@elevation,
                     row.names = st_names)
tmin = exampleinterpolationdata@MinTemperature
tmax = exampleinterpolationdata@MaxTemperature                     
prec = exampleinterpolationdata@Precipitation 
rhum = exampleinterpolationdata@RelativeHumidity
```

Before starting using the package, you need to have access to the elevation (in m) and daily weather data series corresponding a set of locations (normally weather stations). Elevation is needed because interpolation routines perform corrections for differences in elevation between the reference locations and the target point. The initial format of your data will be different depending on the format used by your data provider (the package has also tools to access weather data). For our example, we will assume you have data from a set of 38 stations in your study area. On one hand, you should have a `data.frame` with the coordinates and elevation of each location:
```{r}
str(st_data)
head(st_data)
```
On the other, you should have at least three matrices of meteorological data (one for minimum temperature, one for maximum temperature and the last one for precipitation) with stations in rows and dates in columns. In our example we also add relative humidity (in percent), so that other derived variables can be calculated:
```{r}
dim(tmax)
dim(tmin)
dim(prec)
dim(rhum)
tmax[1:6,1:6]
```
Units should be in degrees Celsius for temperature and mm for precipitation.

## Building an interpolation data object

Package **meteoland** stores weather series for reference locations and interpolation parameters in a single object of class `MeteorologyInterpolationData`. There are several ways of building such objects, but we will first illustrate how to do it from the data we just presented.

First we need to create an object of class `SpatialPoints` (see package **sp**) with the spatial coordinates of our weather stations and the coordinate system (here UTM 31N):
```{r}
sp = SpatialPoints(st_data[,c("X_UTM", "Y_UTM")],
                   proj4string = CRS("+proj=utm +zone=31 +ellps=WGS84 +datum=WGS84 +units=m +towgs84=0,0,0"))
head(sp)
```
We can now build an object `MeteorologyInterpolationData` using:
```{r}
interpolator <- MeteorologyInterpolationData(sp, elevation = st_data$elevation,
                                             MinTemperature = tmin,
                                             MaxTemperature = tmax,
                                             Precipitation = prec,
                                             RelativeHumidity = rhum)
class(interpolator)
```

The resulting object is ready to be used to perform interpolation on a set of target locations (see next section). We can inspect the amount of data in our interpolation object using function `interpolation.coverage`. For example, with:
```{r}
spatial_coverage <- interpolation.coverage(interpolator, type = 'spatial')
head(spatial_coverage)
```
we obtain the number of non-missing observations for each weather station and variable (i.e. the spatial coverage). Similarly, we can ask the number of non-missing observations for each date and variable (i.e. the temporal coverage) using:
```{r}
temporal_coverage <- interpolation.coverage(interpolator, type = 'temporal')
head(temporal_coverage)
```
 
Interpolation parameters are also stored in the same object (see next subsection):
```{r}
names(interpolator@params)
```



## Interpolation basics and parameters
Package meteoland implements, with a few modifications, the daily weather interpolation and estimation algorithms that un- derpin the U.S. [DAYMET](https://daymet.ornl.gov/) dataset (Thornton et al., 1997; Thornton and Running, 1999).This approach, similar to inverse distance weighting, interpolates weather variables using trun- cated Gaussian filters, which consist in defining spatial weights $W(r)$ at radial distance $r$ from a target point $p$ using:
\begin{equation}
W(r) = e^{-\alpha \cdot (r/R_p)^2} - e^{-\alpha}
\end{equation}
if $r \leq R_p$ and $W(r) = 0$ otherwise. 

Here $r$ is the radial distance from $p$, $R_p$ is the truncation distance and $\alpha$ is the **shape** parameter. The spatial convolution of this filter with a set of weather station locations results, for each target point, in a vector of weights associated with observations. The following figure illustrates the Gaussian filter for $R_p = 500$ and either $\alpha = 3.0$ (continuous line) or $\alpha = 6.25$ (dashed line):

```{r, echo = FALSE, fig = TRUE, fig.width=6, fig.height=4}
r = 0:1000
R_p = 500
gf1 = exp(-3.0*((r/R_p)^2.0)) - exp(-3.0)
gf2 = exp(-6.25*((r/R_p)^2.0)) - exp(-6.25)
gf1[r>R_p] = 0
gf2[r>R_p] = 0
plot(r, gf1, type="l", ylab = "W(r)", xlab ="r")
lines(r, gf2, lty=2)
legend("topright", legend = c("alpha = 3", "alpha = 6.25"), lty=c(1,2), bty="n")

```

$R_p$ is automatically adjusted so that it has lower values in data-rich regions and is increased in data-poor regions. The method, however, requires the user to specify $N$, the average number of observations to be included for each target point. $R_p$ is then varied as a smooth function of the local density in such a way that this average is achieved over the spatial domain. It is important that the initial value of $R_p$ 

In meteoland estimation of $R_p$ is done once for each target point, variable and day. Interpolation of temperature includes a correction for the effects of elevation. More specifically, a weighted least-squares regression is used to assess the relationship between temperature differences and elevation differences in weather station data and this relationship is applied to elevation differences between weather stations and the target point. Interpolation of relative humidity is done after transforming it to dew-point temperature. No correction for elevation is performed during interpolation, but elevation effects arise when back-transforming dew-point temperature to relative humidity. Interpolation of daily precipitation is complicated by the need to predict both precipitation occurrence and, conditioned on this, precipitation amount. Thornton et al. (1997) defined a binomial predictor of spatial precipitation occurrence as a function of the weighted occurrence at surrounding weather stations. Conditional on precipitation occurrence, the interpolation routine predicts precipitation amount, where weighted least-squares regression is also used to account for elevation effects. Interpolation of wind is performed in three different ways depending on the information available. If only wind speed data is available, the spatial interpolation with Gaussian weights is used on wind scalars as described above. If weather station data includes wind direction, a polar average is cal- culated using Gaussian weights. Finally, if static wind fields are also available the interpolation routine first finds, for each weather station the wind field that best matches the observed vector. Then, the wind vectors extracted from the selected wind fields are averaged as before. Further details of how interpolation is done can be found [vegmod website](http://vegmod.ctfc.cat/software/meteoland/).

Interpolation parameters $\alpha$ and $N$ can be different for each variable to be interpolated. The following table lists all the interpolation parameters (see also function `defaultInterpolationParameters()`)

| Paremeter      | Default value | Definition                          |
| ------------- | ---------- | ----------------------------------- |
| `initial_Rp` | 140000 | Initial truncation radius |
| `iterations` | 3      | Number of station density iterations |
| `alpha_MinTemperature` | 3.0 | Gaussian shape parameter for minimum temperature |
| `alpha_MaxTemperature` | 3.0 | Gaussian shape parameter for maximum temperature |
| `alpha_DewTemperature` | 3.0 | Gaussian shape parameter for dew-point temperature |
| `alpha_PrecipitationEvent` | 5.0 | Gaussian shape parameter for precipitation events |
| `alpha_PrecipitationAmount` | 5.0 | Gaussian shape parameter for the regression of precipitation amounts |
| `alpha_Wind` | 3.0 | Gaussian shape parameter for wind |
| `N_MinTemperature` | 30 | Average number of stations with non-zero weights for minimum temperature |
| `N_MaxTemperature` | 30 | Average number of stations with non-zero weights for maximum temperature |
| `N_DewTemperature` | 30 | Average number of stations with non-zero weights for dew-point temperature |
| `N_PrecipitationEvent` | 5 | Average number of stations with non-zero weights for precipitation events |
| `N_PrecipitationAmount` | 20 | Average number of stations with non-zero weights for the regression of precipitation amounts |
| `N_Wind` | 2 | Average number of stations with non-zero weights for wind |
| `St_Precipitation` | 5 | Number of days for the temporal smoothing of precipitation |
| `St_TemperatureRange` | 15 | Number of days for the temporal smoothing of temperature range |
| `pop_crit` | 0.50 | Critical precipitation occurrence parameter |
| `f_max` | 0.6 | Maximum value for precipitation regression extrapolations (0.6 equals to a maximum of 4 times extrapolation) |
| `wind_height` | 10 | Wind measurement height (in m) |

Parameter `St_Precipitation` controls the temporal smoothing that is applied to weather station data to calibrate regression, while parameters `pop_crit` and `f_max` are also particular to the estimation of precipitation (see details in Thornton et al. 1997). Parameter `St_TemperatureRange` is used for the estimation of solar radiation.

A parameter that is particularly important to understand is `initial_Rp`, which specifies the initial radius for the truncated spatial Gaussian kernel. By default its value is:
```{r}
interpolator@params$initial_Rp
```
The value of `initial_Rp` must be set in relation to the units of the spatial coordinates of weather data. Our data was in meters, so the default radius is 140 km. In general, the initial radius should be large enough to include a reasonable number of stations (~20-40), but the kernel radius is adjusted for each interpolation target point.

## Calibration and cross-validation of the interpolation data
Once we already have weather stations data in shape, we can start calibrating the model in order to obtain the optimal parameters for the meteorological variables we want to interpolate. Parameter calibration has to be done for each variable separately. For example for minimum temperature:
```{r}
tmin_cal <- interpolation.calibration(interpolator, variable = "Tmin",
                                      N_seq = 20,
                                      alpha_seq = seq(5, 10, by = 1),
                                      verbose = TRUE)
```

This function returns an interpolation.calibration class object which contains several items:

* Numeric matrix with the mean absolute error (MAE) values for each combination of parameters $N$ and
$\alpha$.
* Miminum value found for MAE.
* Value for the `N` parameter corresponding to the minumun MAE.
* Value for the `alpha` parameter corresponding to the minimum MAE.
* Matrix with the observed values.
* Matrix with the predicted values for the optimum parameter combination.

The result of the calibration needs to be manually stored in the interpolation params:
```{r}
interpolator@params$N_MinTemperature = tmin_cal$N
interpolator@params$alpha_MinTemperature = tmin_cal$alpha
```

We strongly recommend conducting calibration exercises at least once for each variable and each data set used as reference for interpolation, and more than once if periods differ in the number of stations available.

Before using the object for interpolations, we also need to assess its performance. This is done by cross-validation in function `interpolation.cv`:
```{r,echo=FALSE}
cv <- interpolation.cv(interpolator, verbose=T)
```

Cross-validation is perfomed by *leave-one-out*, which means that each target station is first removed from the data set and then the remaining stations are used to obtain interpolation estimates. In this way one maximizes the amount of information for estimates, while keeping them independent of the observed values in each station. The results of cross-validation can be inspected using a specific `summary` function:
```{r}
summary(cv)
```

## Interpolation on a grid
```{r, echo = FALSE, include= FALSE}
data("examplegridtopography")

elev = as(examplegridtopography[1:20,1:20], "SpatialGridDataFrame")["elevation"]
```
The target for weather interpolation in **meteoland** can be a set of points, pixels or a whole grid. Again, the initial format of data can be very different. Here we assume you have a small grid of 400 (20x20) cells of 1ha in size, with elevation data in form of class `SpatialGridDataFrame` (see method `read.asciigrid` in package *sp*):
```{r}
summary(elev)
```

Note that the coordinate reference system needs to be the same as that of `interpolator`, which in this case it is. Before performing the interpolation over this grid, we need to reshape this data in a class called `SpatialGridTopography`:
```{r}
sgt = SpatialGridTopography(as(elev, "SpatialGrid"), elevation = elev$elevation,
                            proj4string = elev@proj4string)
sgt
```

As you can see in the result, **meteoland** has calculated for us slope and aspect (both in degrees) from elevation data. Objects of class `SpatialGridTopography` can be initialized with user input values for slope and aspect too, but **meteoland** has its own routines when this are missing]. Slope and aspect are important for radiation calculations, which also requires relative humidity data. We can display elevation over the grid using:
```{r}
spplot(sgt, "elevation")
```


Before we call the interpolation routine, we need to define the dates (i.e. days) for which we want weather to be interpolated, for example:
```{r}
dates = as.Date(c("2001-02-03", "2001-06-03"))
```

Of course, we need to be sure that the `interpolator` object has data corresponding to this dates. We can check if there is any missing date using:
```{r}
sum(!(dates %in% interpolator@dates))
```

The name of interpolation functions depend on the target spatial structure. For grids we need to use function `interpolationgrid`:
```{r}
ml <- interpolationgrid(interpolator, sgt, dates)
```

This function works processing each date at a time. Since calculations can take some time, the console output shows the progress. The output of the function is an object of class `SpatialGridMeteorology`:
```{r}
ml
```
We can display interpolated grids in a map using function `spplot`:
```{r, fig.show="hold"}
spplot(ml, 2, "MinTemperature")
spplot(ml, 2, "MaxTemperature")
```

Objects of class `SpatialGridMeteorology` include a list of data frames, one per date. We can access the interpolated data for a given date using:
```{r}
df_1 = ml@data[[1]]
head(df_1)
```

Some columns are missing (e.g. wind speed) because we did not include weather station data regarding these variables. If we wants to add grid coordinates to this data frame, we can use the spatial information stored in the `ml` object:

```{r}
sgdf_1 = SpatialGridDataFrame(grid = ml@grid, data = ml@data[[1]], proj4string = ml@proj4string)
summary(sgdf_1)
```

Results can be retrieved in this way and saved using `write.asciigrid` for its use outside R. The package also provides function for reading/writing NetCDFs (see function `writemeteorologygrid`) from `SpatialGridMeteorology` objects. Finally, the package allows interpolating on subsets of grid pixels in the same way as for full grids. This is done using objects of class `SpatialPixelsTopography` and calling function `interpolationpixels`, which will produce objects of class `SpatialPixelsMeteorology`.


## Interpolation on a set of points
```{r, echo = FALSE, include= FALSE}

spt = as(examplegridtopography, "SpatialPointsTopography")[c(36,228, 530, 2304)]
cc = coordinates(spt)
points_df = data.frame(X_UTM = cc[,1], Y_UTM = cc[,2], elevation = spt@data$elevation)
```
If you want to interpolate on a set of target locations, the starting point will normally be a `data.frame`. In our example this points come from the grid, but we have reshaped them so the starting format is familiar:
```{r}
points_df
```

Analogously with the grid, we need to transform this data into an object `SpatialPointsTopography`:
```{r}
spt = SpatialPointsTopography(as.matrix(points_df[,c("X_UTM", "Y_UTM")]),
                              elevation = points_df$elevation,
                              proj4string = CRS("+proj=utm +zone=31 +ellps=WGS84 +datum=WGS84 +units=m +towgs84=0,0,0"))
spt
```

In this case we only have elevation (in m), but slope and aspect should also be included if possible. Let us assume you want to interpolate on this points for the whole time series available in object `interpolator`. Since we are dealing with points, the function to interpolate is called `interpolationpoints`:
```{r}
mp = interpolationpoints(interpolator, spt)
```
This function works processing one point at a time. The output of the function is an object of class `SpatialPointsMeteorology`:
```{r}
mp
```

And the time series for a given can be plotted using function `meteoplot`. For example, we show here the precipitation series of point #1:
```{r, fig =TRUE, fig.width=7, fig.height=5}
meteoplot(mp, 1, "Precipitation", ylab="Precipitation (mm)", xlab="")
```

Objects of class `SpatialPointsDataFrame` include a list of data frames, one per point. We can access one of them using:
```{r}
df_1 = mp@data[[1]]
head(df_1)
```

This data frame can now be written into a file for its analysis outside R. The package also provides its own functions to write/read point meteorology data in different formats. If we are interested in inspecting the interpolation result by date, instead of by point, we can use function `extractdates`, which returns objects of class `SpatialGridDataFrame`:
```{r}
dt_4 = extractdates(mp, as.Date("2001-01-04"), verbose = FALSE)
dt_4
```

# Statistical correction of daily weather

Correcting the biases of a meteorological data series containing biases using a more accurate meteorological series is necessary when the more accurate series does not cover the period of interest and the less accurate series does. The less accurate series may be at coarser scale, as with climate model predictions or climate reanalysis data. In this case one can speak of statistical correction and downscaling. However, one may also correct the predictions of climate models using reanalysis data estimated at the same spatial resolution.

In the following example we will correct the predictions of Regional Climate Model (CCLM4-8-17; driving global model CNRM-CERFACS-CNRM-CM5) on the same area of the interpolation example. RCM data includes 3 model cells. Meteorological data covers an historical (reference) period (2000-2003) and a future (projection) period (year 2023), the latter simulated under rcp4.5 scenario.

## Preparing weather data to be downscaled/corrected

```{r, echo = FALSE, include= FALSE}
data("examplecorrectiondata")
coords = examplecorrectiondata@coords
pt_coords = data.frame(long = as.numeric(coords[,1]), lat = as.numeric(coords[,2]))
proj_dates = examplecorrectiondata@dates
ref_data = examplecorrectiondata@reference_data
proj_data = examplecorrectiondata@projection_data
```

One needs several data items to perform downscaling and statistical correction. First, we need a matrix or data frame with the central coordinates of the RCM cells (here in longitude/latitude format):
```{r}
pt_coords
```
Second, we need the uncorrected meteorological data (here RCM outputs) for both a reference period (that will be matched with our more accurate series) and a projection period (that our more accurate series does not cover). Both should be arranged in lists of data frames, one per RCM cell:
```{r}
length(ref_data)
length(proj_data)
head(ref_data[[1]])
head(proj_data[[1]])
```
Note that these data frames should follow the conventions of **meteoland** for variable names and units. Finally, we need to specify the projection period, in this case one year:
```{r}
proj_dates = seq(as.Date("2023-01-01"), as.Date("2023-12-31"), by="day")
```

## Building the uncorrected data object

Statistical correction needs an object of class `MeteorologyUncorrectedData`, analogous to the `MeteorologyInterpolationData` of the previous section. To build this object we need first to express coordinates in an object `SpatialPoints`:
```{r}
sp = SpatialPoints(pt_coords, CRS("+proj=longlat +datum=WGS84 +ellps=WGS84 +towgs84=0,0,0"))
sp
```

Assuming the weather data to be corrected is in the proper format, the object is constructed using:

```{r}
uncorrected = MeteorologyUncorrectedData(sp, ref_data, proj_data, proj_dates)
```

## Target point weather meteorology taken as reference

Downscaling/statistical correction is done on a set of target spatial points. meteoland will first find the RCM cell to which each point is nearest (using the central coordinates of RCM cells). Once this matching is done, statistical relations are build between the meteorology of RCM cells and that of target points for the reference period (here 2000-2003) which are used to correct RCM data for the projection period (year 2023). For this process to be done, we need the coordinates and weather series for the reference period. In our case, we will employ a copy the object of class `SpatialPointsMeteorology` that resulted from interpolation in the previous section:
```{r}
historical  = mp
historical
```
We named it `historical` to remind that we are using the historical period as reference and want to correct the RCM series for the projection period There are several ways to shape data into objects of class `SpatialPointsMeteorology`. For example, one can use  function `readmeteorologypoints`. 

## Tuning correction parameters

Objects of class `MeteorologyUncorrectedData` have a slot with parameters:
```{r}
uncorrected@params
```
Importantly, `varmethods` is a named list that specifies which correction method has to be used for each variable. Since we do not have reference data for wind speed, we must turn the method for wind speed to `"none"`:
```{r}
uncorrected@params$varmethods$WindSpeed="none"
```


## Conducting statistical correction
Once we have all the data objects that we need (the hard part), conducting statistical correction is straightforward:
```{r}
projected = correctionpoints(uncorrected, historical)
```
As mentioned above, correction proceeds point by point. The result is again an object of class `SpatialPointsMeteorology`:

```{r}
projected
```

The following code displays the minimum/maximum temperatures before and after correction:
```{r, fig=TRUE, fig.width=7, fig.height=5}
#Plot predicted mean temperature for point 1
meteoplot(projected, 1, "MinTemperature", ylab="Temperature (Celsius)", ylim=c(-5,40), col="blue")
meteoplot(projected, 1, "MaxTemperature", add=TRUE, col="red")
#Add uncorrected mean temperature data (cell #3)
lines(uncorrected@dates,
      uncorrected@projection_data[[3]]$MinTemperature,
      col="blue", lty=3)
lines(uncorrected@dates,
      uncorrected@projection_data[[3]]$MaxTemperature,
      col="red", lty=3)
legend("topright", legend=c("corrected","uncorrected", "Maximum", "Minimum"), 
       col=c("black","black", "red","blue"), lty=c(1,3,1,1), bty="n")

```

# Stochastic weather generation

Recent versions of **meteoland** incorporate the possibility of generating stochastic weather series. Stochastic weather generators are algorithms that produce series of synthetic daily weather data. The parameters of the model are conditioned on existing meteorological records to ensure the characteristics of input weather series emerge in the daily stochastic process. The algorithm available in **meteoland** is intended to be used to generate daily series of the same length as the input. It can be understood as a resampling algorithm that tries to preserve some properties of the input series. The algorithm is semi-parametric and based on a first-order Markov chain for weather days (classified into dry/wet/extreme wet) along with k-nearest neighbour (KNN) resampling of input days and years. The approach implemented in **meteoland** can be applied to any spatial structure (points/pixels/grid) and it preserves the spatial correlation and multivariate covariance structure of weather series (because it works on area-averaged weather and the chosen resampled days are applied to all points/pixels). 

## Weather generation function

Function `weathergeneration` can be used to generate synthetic weather series for a range of inputs, including a (non-spatial) data frame (corresponding to weather series of a single location) as well as objects of classes `SpatialPointsDataFrame`, `SpatialPixelsDataFrame` or `SpatialGridDataFrame`. The following calls the function with a `SpatialPointsDataFrame` object, while hiding console output:

```{r}
y <- weathergeneration(mp, verbose=FALSE)
```
The output of the function is of the same class as the input object:

```{r}
class(y)
```

We use the following code to display the original and synthetic temperature and precipitation values at the monthly scale:
```{r, fig =TRUE, fig.width=7, fig.height=7, echo = TRUE}
par(mar=c(3,5,1,1), mfrow = c(2,1))
meteoplot(mp, 1, "MeanTemperature", freq="months", fun="mean", ylab="Mean temperature (Celsius)", xlab="")
meteoplot(y, 1, "MeanTemperature", freq="months", fun="mean", col="red", add=T)
legend("bottomright", legend = c("original", "synthetic"), col=c("black", "red"), lty=1, bty="n")
meteoplot(mp, 1, "Precipitation", freq="months", fun="sum", ylab="Precipitation (mm/month)", xlab="")
meteoplot(y, 1, "Precipitation", freq="months", fun="sum", col="red", add=T)
legend("bottomright", legend = c("original", "synthetic"), col=c("black", "red"), lty=1, bty="n")
```


## Weather generation parameters

One of the inputs of function `weathergeneration` is an list with algorithm parameters. The names of these parameters, and their default values, can be obtained from function `defaultGenerationParameters()`:
```{r}
defaultGenerationParams()
```

Among all parameters, the most important is `$conditional`, as it specifies the multiyear conditioning of the generated series:

1. **"none"** - The non-conditional version is used, which is based on a first order Markov chain (MC) to simulate weather states (dry/wet/extreme wet) and a K-nearest neighbour (KNN) algorithm to select pairs of days with the same transition and similar weather for the initial state (as in Apipattanavis et al. 2007).
2. **"arima"** - Annual precipitation is conditioned using a stationary auto-regressive (ARIMA) model and then a K-nearest neighbour algorithm is used to select a set of years to train the MC-KNN algorithm (similar to Steinschneider et al. 2013). Recommended if low-frequency variation of annual precipitation is to be acounted for in long series.
3. **"window"** - The MC-KNN algorithm is trained with the subset of the input data corresponding to a window around the target year. Annual precipitation is conditioned using a lognormal random trial of the precipitation corresponding to the selected years. Recommended to generate stochastic series from climate change projections.
