# Quadrangle Mesh

## Documentation for package ‘quadmesh’ version 0.4.5

- DESCRIPTION file.
- User guides, package vignettes and other documentation.

## Help Pages

bary_index | Barycentric triangle index for interpolation
dquadmesh | Create a quad-type mesh for use in rgl.
dquadmesh.default | Create a quad-type mesh for use in rgl.
dtriangmesh | Create a triangle-type mesh for use in rgl.
dtriangmesh.default | Create a triangle-type mesh for use in rgl.
etopo | World topography map
llh2xyz | Angular coordinates to X, Y, Z.
mesh_plot | Plot as a mesh
mesh_plot.BasicRaster | Plot as a mesh
mesh_plot.mesh3d | Plot as a mesh
mesh_plot.quadmesh | Plot as a mesh
mesh_plot.RasterLayer | Plot as a mesh
mesh_plot.stars | Plot as a mesh
mesh_plot.TRI | Plot as a mesh
qm_as_raster | Quadmesh to raster
qsc | Quadrilateralized Spherical Cube (QSC)
quadmesh | Create a quad-type mesh for use in rgl.
quadmesh.BasicRaster | Create a quad-type mesh for use in rgl.
quadmesh.matrix | Create a quad-type mesh for use in rgl.
triangmesh | Create a triangle-type mesh for use in rgl.
triangmesh.BasicRaster | Create a triangle-type mesh for use in rgl.
triangmesh.matrix | Create a triangle-type mesh for use in rgl.
triangulate_quads | Triangles from quads
use_crs | In-use coordinate system
worldll | World raster map
xymap | World map