# Image Tools for Automated Wood Identification

## Documentation for package ‘wvtool’ version 1.0

- DESCRIPTION file.

## Help Pages

bin2dec | Binary Number to Decimal number Conversion
camphora | Image Sample Dataset
car2pol | Polar Transformer -Cartesian to Polar Coordinates-
cc.label | Connected Component Labelling.
crop | Image cropping
cryptomeria | Image Sample Dataset
dec2bin | Decimal to Binary Convertion
edge.detect | Canny and Sobel Edge detector.
gabor.filter | Two Dimensional Gabor Filtering in Frequency Domain
glcm | Gray Level Co-occurence Matrix (glcm)
gray2bin | Conversion from Grayscale to Binary Image
haralick | Haralick Texture Features Calculated from GLCM
hlac | Higher Order Local Autocorrelation (HLAC)
integ.profile | Simple Integration for Making Profile
lbnum | Counts 0-1 or 1-0 in a Binary Sequence
lbp | Local Binary Patterns (lbp)
noise.filter | Median, Mean and Gaussian Filter
rgb2gray | Convert RGB image to Grayscale
rot90c | Transpose Image 90 Degrees Clockwisely
rotate.matrix | Image Rotation by Bilinear Interpolation
swap.quad | Swapping Quadrants